BMP280

* Interface I2C ( Vin = 5v, GND = GND , SCK=21 , SDI=20)
* Can give take both the temperature and pressure values
* Libraries: Wire , Adafruit\_BMP280 , SPI
* #define BMP\_SCK  (52)
* #define BMP\_MISO (50)
* #define BMP\_MOSI (51)
* #define BMP\_CS   (10)